B o s e i  M a r u  2  B r i d g e  D a t a  Q u a l i t y C o n t r o l  R e p o r t David F. Zierden and Shawn R. SmithW o r l d  O c e a n  C i r c u l a t i o n  E x p e r i m e n t  ( W O C E ) Surface Meteorological Data Assembly CenterCenter for Ocean Atmospheric Prediction StudiesFlorida State UniversityDecember 21, 2000Report WOCEMET 97-18Version 2.0

Addendum:Member�s of the WOCE Hydrographic Project Office (WHPO) and WOCEMET met at the 13thData Products Committee (DPC) meeting in College Station, TX to discuss reconciliation of theWOCE cruise line designators. This was done in anticipation of the future release of version 3 ofthe WOCE global data set, and resulted in changes to several WOCE cruise line designations.On December 21, 2000, WOCEMET changed the WOCE designator for the cruise P__02W/00 tothe updated form, P__02C/00.2

Introduction:This report summarizes the quality of surface meteorological data collected by the Bosei Maru 2(identifier: JGAW) bridge crew during one WOCE cruise. The data were provided to the FloridaState University Data Assembly Center (DAC) in electronic format by M. Fukasawa at TokaiUniversity, Japan. They were converted to standard DAC netCDF format. The data were thenprocessed using an automated screening program which adds quality control flags to the data,highlighting potential problems. Finally, the Data Quality Evaluator reviews the data and currentflags. Flags are then added, modified, and deleted according to the judgement of the Data QualityEvaluator and other DAC personnel. An in depth description of the WOCE quality controlprocedures can be found in Smith et al. (1996). The data quality control report summarizes allflags for the Bosei Maru 2 bridge data and explains reasons why these flags were assigned.Statistical Information:The Bosei Maru 2 data are expected to include observations taken every hour on the WOCE cruise.Values for the following variables were collected:Time(TIME)Latitude(LAT)Longitude(LON)Ocean Relative Wind Direction(DIR)Ocean Relative Wind Speed(SPD)Sea Temperature(TS)Atmospheric Pressure(P)Air Temperature(T)Relative Humidity(RH)Total Cloud Amount(TCA)* * Checked only for correct WMO coding.Details of the cruise including cruise dates, number of records, number of values, number of flags,and percentage flagged are listed in Table 1. A total of 2,529 values are evaluated with 1 flag 3 added by the preprocessor and Data Quality Evaluator for a total of 0.04 percent of the values beingflagged.Table 1: Statistical Cruise InformationCTC

Dates

Number of

Records

Values

Flags

Percentage

Flagged

P__02W/0001/20/94 - 02/02/94

2812,529

10.04

Summary:The bridge data for the Bosei Maru 2 are of excellent quality. Only one flag was assigned in theentire data set, an �S� for a solitary spike in sea temperature. The only variable of concern is winddirection, which was only measured to the nearest 22.5 degree increment. DIR data may not besufficiently accurate to fulfill the user�s purposes. All the other variables seem to be very reliableand should present no problems for the user.References:Smith, S. R., C. Harvey, and D. M. Legler, 1996: Handbook of Quality Control Procedures andMethods for Surface Meteorology Data. WOCE Report No. 141/96, Report WOCEMET96-1, Center for Ocean Atmospheric Prediction Studies, Florida State University,Tallahassee, FL 323014