Sogen Maru Standard BridgeObservations Data Quality ControlR e p o r t Cruises: PR_01S/01 PR_23_/01David F. Zierden and Shawn R. SmithWorld Ocean Circulation Experiment (WOCE)Surface Meteorological Data Assembly CenterCenter for Ocean Atmospheric Prediction StudiesFlorida State UniversityFebruary 24, 1997Report WOCEMET 97-11Version 1.0

Introduction:The data referenced in this report were collected from the research vessel Sogen Maru (Call sign:JNQK; Data Provider: unknown/ H. Watanabe) standard bridge observations for one cruisecovering two WOCE hydrographic lines. These data were received by the Data Assembly Center(DAC) in electronic format and converted to a standard FSU format. They were then preprocessedusing an automated data checking program. Next the Data Quality Evaluator completed a visualinspection and reviewed, modified, and added appropriate Quality Control (QC) flags to the data.Details of the WOCE QC procedures can be found in Smith et al (1996). The data quality controlreport summarizes the flags for the Sogen Maru standard bridge observations, including thoseadded by both the preprocessor and the Data Quality Evaluator.Statistical Information:The data referenced in this report were expected to include observations taken every 4 hours by theSogen Maru bridge crew. The details of the cruise including start and end date, number of values,number of records, number of flags, and percentage are presented in table 1.Table 1: Statistical Cruise InformationCTC Dates

Number of

Records

Values flags

Percentage

Flagged

PR_01S/01

PR_23_/0101/04/91 -

01/11/91

352450Time (TIME), latitude (LAT), longitude (LON), earth relative wind direction (DIR), earth relativewind speed (SPD), atmospheric pressure (P), and air temperature (T) were the variables analyzed.A total of 245 values were checked with no flags added by the preprocessor of the Data QualityEvaluator.2

Summary:The standard bridge observations from the Sogen Maru proved to be very reliable. No values wereflagged by the prescreener and the visual inspection revealed no other problems with the data.Final Note:These data are in outstanding condition and should present no problems for the user.References:Smith, S. R., C. Harvey, and D. M. Legler, 1996: Handbook of Quality Control Procedures andMethods for Surface Meteorology Data. WOCE Report No. 141/96, Report WOCEMET96-1, Center for Ocean Atmospheric Prediction Studies, Florida State University,Tallahassee, FL 32301.3